|  |  |  |
| --- | --- | --- |
|  |  |  |

**Students Innovative Project Report**

**DESIGN AND DEVELOPMENT OF IOT BASED PORTABLE BIOMEDICAL KIT FOR HEPATITIS AND JAUNDICE**

**SIP ID -2122S4482**

Submitted by

**SANTHOSH KUMAR. V. M – 810019105074**

**ROHITH. P – 810019105067**

**SAKTHIVEL. S – 810019105071**

Guided by

**Dr. P. ANBALAGAN**

**DEPARTMENT OF ELECTRICALAND ELECTRONICS ENGINEERING,**

**BHARATHIDASAN INSTITUTE OF TECHNOLOGY (BIT) CAMPUS, TIRUCHIRAPPALLI - 620 024.**

**Anna University**

Sponsored by

**Centre for Sponsored Research and Consultancy (CSRC)**

**Anna University, Chennai – 600 025.**

**DEPARTMENT OF ELECTRICALAND ELECTRONICS ENGINEERING,**

**BHARATHIDASAN INSTITUTE OF TECHNOLOGY (BIT) CAMPUS, TIRUCHIRAPPALLI - 620 024.**

**Anna University**

## BONAFIDE CERTIFICATE

Certified that this project Report titLED “**DESIGN AND DEVELOPMENT OF IOT BASED PORTABLE BIOMEDICAL KIT FOR HEPATITIS AND JAUNDICE"** is submitted by Mr. Sakthivel .S , Mr. Rohith .P , Mr. Santhosh Kumar .V.M who carried out the work under our supervision. Certified further that to the best of my knowLEDge the work reported herein all the guidelines prescribed by the University was followed during and after implementation of the project.

**SIGNATURE OF MENTOR**

**(Dr. P. ANBALAGAN)**

**ACKNOWLEDGEMENT**

I would like to express my special gratitude and thanks to "CSRC-CENTRE FOR SPONSORED RESEARCH AND CONSULTANCY" for giving us such a wonderful opportunity.

A special mention to our dean "Dr . T. Senthilkumar" for supporting us throughout this journey.

Our thanks and appreciations also goes to our HOD "Dr . P. Anbalagan " Dept. Of Electrical and Electronics Engineering in developing the project and we also highly indebted to his guidance and constant supervision as well as for providing necessary information regarding the project & also for his support in completing the project. I would like to express my gratitude towards member of Anna University Regional Campus Tirucjirappalli for their kind co-operation and encouragement which help me in completion of this project.

**SANTHOSH KUMAR V M**

**ROHITH P**

**SAKTHIVEL S**

**ABSTRACT**

Bilirubin is a compound which is yellow in shade, happens within the ordinary catabolic pathway is the breakdown made of heme in vertebrates. This catabolism is a necessary technique inside the body's clearance of waste merchandise that get up from the destruction of aged red blood cells. There are two types of bilirubin namely Conjugated (direct) Bilirubin and Unconjugated (oblique) Bilirubin. The un-conjugated Bilirubin is Albumin-bound in serum and by no means present in urine whereas Conjugated Bilirubin is unbounded in serum and it's miles present in urine. Our proposed concept is set to determine the amount of Conjugated Bilirubin in urine. A medical kit is a collection of supplies and equipment that is used for providing medical care, especially in situations where advanced medical facilities may not be available. It can include items such as bandages, dressings, gauze, adhesive tape, scissors, tweezers, antiseptic wipes, pain medication, and other items that may be needed to provide first aid or treat minor injuries. Some medical kits are designed for specific purposes, such as survival kits or kits for travellers, while others are mare general purpose. It is important to have a medical kit on hand in case of emergencies, and to make sure that the supplies are regularly checked and replenished as needed.

A urine analysis device is a tool that is used to test urine for various chemical and biological markers. These markers can provide information about a person's health and can help diagnose or monitor various medical conditions. There are several types of urine analysis devices available, including Dipsticks, cups or bottles and testing devices.

Testing devices are portable devices that can be used to test a urine sample on the spot. They typically use a combination of chemicals and sensors to detect the presence of various markers in the urine. It is important to follow the manufacturer's instructions when using a urine analysis device, as the accuracy of the results can depend on proper use of the device. There are several methods for performing a bilirubin analysis, including spectrophotometry, which measures the amount of light absorbed by the bilirubin, and immunoassays, which use antibodies to measure the amount of bilirubin in a sample. The specific method used may depend on the type of bilirubin being measured and the equipment available.

We build here a easy electronic circuit fashioned of Light-emitting diodes and light dependent resistors that may be used for analysing bilirubin concentration. We recommend this method due to the fact the BoiLED Rice grains have the capability to absorb Bilirubin pigment. This Biomedical package is used to detect the Jaundice and Hepatitis affected sufferers via quantitative analysis of bilirubin in urine.

**CONTENTS**

|  |  |  |  |
| --- | --- | --- | --- |
| **CHAPTER** |  | **TITLE** | **PAGE NO** |
| 1 |  | Introduction |  |
|  | 1.1 | General | 1 |
|  | 1.2 | Introduction to Urine analysis | 2 |
|  | 1.3 | Rational of Urine analysis | 3 |
|  | 1.4 | Urine | 4 |
|  | 1.5 | Bile | 5 |
| 2 |  | Literature Survey | 7 |
| 3 |  | Concept of existing model | 9 |
| 4 |  | Proposed model of Diagnostic Device | 12 |
| 5 |  | Implementation of proposal device | 15 |
| 6 |  | Hardware Description |  |
|  | 6.1 | Light Dependent Resistor (LDR) | 19 |
|  | 6.2 | Light Emitting Device (LED) | 22 |
|  | 6.3 | PIC microcontroller | 28 |
|  | 6.4 | Internet Of Things (IOT) | 43 |
|  | 6.5 | Power supply | 55 |
|  | 6.6 | Transformer | 57 |
|  | 6.7 | Rectifier | 58 |
| 7 |  | Software |  |
|  | 7.1 | Software Description | 62 |
|  | 7.2 | Arduino IDE | 62 |
|  | 7.3 | Arduino Programming | 64 |
| 8 |  | Results & Conclusion | 83 |
| 9 |  | Future Enhancement | 85 |
| 10 |  | Reference | 86 |

**TABLE OF FIGURES**

|  |  |  |
| --- | --- | --- |
| **FIGURE** | **TITLE** | **PAGE NO** |
| 4.1 | Block Diagram Of Implemented Model | 13 |
| 5.1 | Voltage Divider Circuit | 15 |
| 5.2 | Schematic Diagram Of Implemented Model | 16 |
| 5.3 | Prototype Implementation | 17 |
| 6.1 | LDR Circuit Diagram | 19 |
| 6.2 | Construction Of LDR | 20 |
| 6.3 | Working Principle Of LDR | 21 |
| 6.4 | Schematic Diagram Of LDR | 22 |
| **6.5** | **Block Diagram Of LED** | 22 |
| 6.6 | Cross Sectional View Of Diffused LED | 23 |
| 6.7 | Sectional View Of LED | 24 |
| 6.8 | Working Of LED | 24 |
| 6.9 | Features Of LED | 25 |
| 6.10 | Characteristics Of LED At Different Colours | 26 |
| 6.11 | Voltage Divider Formula In LED | 27 |
| 6.12 | Architecture Of Pic Microcontroller | 28 |
| 6.13 | Features Of Pic32 Microcontroller | 29 |
| 6.14 | Pin Diagram Of Pic16f Microcontroller | 34 |
| 6.15 | Circuit Diagram Of Pin 1 | 34 |
| **6.16** | Circuit Diagram Of Pin 14 | 36 |
| 6.17 | Architecture Of Pic16f Microcontroller | 39 |
| 6.18 | Digital Variable Speed-Limit Sign | 48 |
| 6.19 | Input And Output Ports Of Pic16f Microcontroller | 51 |
| 6.20 | Schematic Of Nodemcu | 52 |
| 6.21 | Features Of Nodemcu | 54 |
| 6.22 | Block Diagram Of RPS | 55 |
| 6.23 | Cross Section Of Battery Power Supply | 56 |
| 6.24 | Transformer | 57 |
| 6.25 | Output Waveform | 59 |
| 6.26 | Full Wave Bridge Rectifier | 59 |
| 6.27 | Output Of Bridge Rectifier | 60 |
| 6.28 | Output Of Single Diode Rectifier | 60 |
| 6.29 | Smoothing Curve | 61 |
| 8.1 | Tabulation Of Tested Results | 83 |
| 8.2 | Graphical Results | 84 |